
S T 9 1 3 5 0 A G       M A R A T H O N    SEAGATE
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders        | 2616|  654| 1024
Capacity form/unform  1350/      MB        Heads           6|   16|   64|   16
Seek time   / track  14.0/ 4.0 ms          Sector/track     |   63|   63|   63
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer           107 KB              Landing Zone
Data transfer rate    6.000 MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method     ZBR PRML89                     operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C                 |
Power: sleep          0.1 W     Humidity     %                 |
       standby        0.3 W     Altitude    km                 |
       idle           0.8 W     Shock        g       125       |
       seek           2.5 W     Rotation   RPM      4500
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST91350/91685AG MARATHON 1350SL/1680  QUICK REFERENCE

 Jumper Setting
 ==============


                            TOP       +- 44-pin I/O Connector
                                      |                     o o
                                    ::::::::::::*::::::::1  o o
                              --P-W-A-----------+-----------+-+----
                                                |           | |
       pin-20 removed for keying ---------------+           | |
                                                            | |
                                                            | |
 Drive is Master, no Slave drive present ------------------ 0 0
 Drive is Master, Seagate Slave drive present ------------- 1 0
 Drive is Slave to another Seagate 2.5" Master ------------ 0 1
 Cable Select --------------------------------------------- 1 1

 Drive uses +5VDC power supplied to the drive via the interface
 connector. The drive does NOT make use of a +12VDC power line.
 pin-41  +5VDC (Logic)
 pin-42  +5VDC (Motor)
 pin-43  Ground
 pin-44  RESERVED


