
D Y L A - 2 6 4 8 0   T R A V E . 8 G S    IBM
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders    8320|     |     |
Capacity form/unform  6480/      MB        Heads           8|     |     |
Seek time   / track  12.0/ 4.0 ms          Sector/track     |     |     |
Controller           IDE / ATA3            Precompensation
Cache/Buffer           512 KB              Landing Zone
Data transfer rate   10.000 MB/S int       Bytes/Sector      512
                     33.300 MB/S ext UDMA2
Recording method     PRML                           operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 65
Power: sleep          0.1 W     Humidity     %         8 90    |      5 95
       standby        0.3 W     Altitude    km                 |
       idle           2.0 W     Shock        g       125       |    400
       seek           2.6 W     Rotation   RPM      4900
       read/write     2.6 W     Acoustic   dBA
       spin-up        5.0 W     ECC        Bit   SMART
                                MTBF         h
                                Warranty Month        24
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
IBM      DYLA-26480/28100  TRAVELSTAR  JUMPER SETTING



              +--------------------------------------+
              |                                      |
              |                                      |
              |                                      |
              +--------Interface-------------49------+
              |       **********************1 **47 Jumper
              |       *************x********* **48   |
              +------44----------------------50------+
              +                                      +

 Pin position 20 is left blank for secure connector insertion.

 Pin position 49: When grounded, no spin-up at POR when open/pull up,
                  normal spin-up at POR.





**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
IBM      DYLA  TRAVELSTAR  JUMPER SETTING

 Jumper Setting
 ==============

 Drive Address Setting
 ---------------------
 A jumper is available at the interface connector to determine the
 drive address.

 Using Cable Selection, the drive address depends on the condition of
 pin 28 of the AT interface cable. In the case when pin 28 is ground
 or low, the drive is a Master. If pin 28 is open or high level, the
 drive is a Slave.


   ---49--47+
    *   * * | Master
    *   * * | (Default setting)
   ---50--48+

   ---49--47+
    *   * X | Slave
    *   * X |
   ---50--48+

   ---49--47+
    *   * * | Cable Selection
    *   xxx |
   ---50--48+

   ---49--47+
    *   xxx | RESERVED       (MASTER)
    *   * * |
   ---50--48+

   ---49--47+
    *   X * | NEVER ATTACH A JUMPER HERE!
    *   X * |
   ---50--48+


 49-PIN: When grounded, no spin-up at POR
         When open/pull-up, normal spin-up at POR


