
7 4 0 5 A V    MAXTOR
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |  989|     |
Capacity form/unform   405/      MB        Heads           3|   16|     |
Seek time   / track  12.0/ 3.0 ms          Sector/track     |   50|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer            32 KB ON-BOARD     Landing Zone
Data transfer rate    4.750 MB/S int       Bytes/Sector      512
                     11.100 MB/S ext PIO3
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 50    |    -40 71
Power: sleep              W     Humidity     %                 |      5 95
       standby            W     Altitude    km    -0.061  3.048|
       idle               W     Shock        g        35       |    120
       seek               W     Rotation   RPM      3551
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
MAXTOR   7405AV  JUMPER SETTING

  +---------------------------------------------------------+
  |                                          J20******J25   |
  |         COMPONENT SIDE                      ******      |XXI
  |                                                         |XXN
  |                                                         |XXT
  |                                                         |XXE
  |                                                         |XXR  J1
  |                                                         |XXF
  |                                                         |XXA
  |                                                         |XXC
  |                                                         |XXE
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |  1
  |                                                         |XX Power
  |                                                         |XX J3
  +---------------------------------------------------------+  1



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MAXTOR   7405AV  JUMPER SETTING

 Jumper Setting
 ==============

 Jumper Designation
 ------------------
     +---------------- J20 Master/Slave
     |  +------------- J21 FACTORY RESERVED!
     |  |  +---------- J22 FACTORY RESERVED!
     *  *  *  *  *  *
     *  *  *  *  *  *
              |  |  +- J25 FACTORY RESERVED!
              |  +---- J24 Cable Select
              +------- J23 Write Cache


 J20 Master/Slave
 ----------------
 J20 CLOSED  Only drive in single drive system (default)
     CLOSED  Master drive in dual drive system (default)
     OPEN    Slave drive in dual drive system


 J23 Write Cache
 ---------------
 J23 OPEN   Write Cache enabled (default)
     CLOSED Write Cache disabled


 J24 Cable Select
 ----------------
 J24 OPEN   Cable Select disabled (default)
     CLOSED Cable Select enabled

 NOTE
 Jumpers J21 and J25 are factory reserved.


 DC Power connector
 ------------------
  pin 1    +12 VDC
  pin 2    +12 Volts Return
  pin 3    + 5 Volts Return
  pin 4    + 5 VDC



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


