
D K 1 1 0 A - 1 3    HITACHI
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 1.8"/SUPERSLIMLINE    Cylinders    1304|     |     |
Capacity form/unform   128/      MB        Heads           4|     |     |
Seek time   / track  16.0/ 6.0 ms          Sector/track     |     |     |
Controller           IDE / AT              Precompensation
Cache/Buffer            32 KB LOOK-AHEAD   Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                      5.000 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 70
Power: sleep              W     Humidity     %        19 90    |      8 90
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |    150
       seek               W     Rotation   RPM      4464
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     250000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


