
E M P I R E   2 1 0 0   W S   S C A    QUANTUM
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    3053|     |     |
Capacity form/unform  2103/      MB        Heads          12|     |     |
Seek time   / track   9.0/ 1.8 ms          Sector/track     |     |     |
Controller           SCSI2/3 WI/SCA/FAST   Precompensation
Cache/Buffer           512 KB LOOK-AHEAD   Landing Zone
Data transfer rate    5.000 MB/S int       Bytes/Sector      512
                     20.000 MB/S ext SYNC
Recording method     PRML 8/9                       operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C           55    |    -40 75
Power: sleep              W     Humidity     %         5 95    |      5 95
       standby            W     Altitude    km    -0.061  3.000| -0.300 12.000
       idle           9.6 W     Shock        g        10       |     60
       seek          12.5 W     Rotation   RPM      5400
       read/write    10.8 W     Acoustic   dBA        37
       spin-up            W     ECC        Bit   112,REED SOLOMON
                                MTBF         h     500000
                                Warranty Month
Lift/Lock/Park     YES          Certificates     CSA,FCC,TUV,UL1950,VDE       

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
QUANTUM  EMPIRE SCA






    It never exist a manual about the SCA disks. Please see the
    Empire description.













